****

Approved by AICTE, New Delhi & Affiliated to JNTUK, Kakinada

Chebrolu (V&M), Guntur (Dt), A.P-522212

|  |  |
| --- | --- |
| **BLOCK :** | **G** |
| **FLOOR :** | **GROUND FLOOR** |
| **ROOM NO:** | **001/CONCRETE TECHNOLOGY LAB** |
| **ROOM SIZE (in Sq. mtrs):** | **41.8** |
| **LAB NAME:** | **CONCRETE TECHNOLOGY LAB** |
| **FANS :** | **1** |
| **TUBE LIGHTS :** | **0** |
| **CHAIRS :** | **1** |
| **STAFF TABLES :** | **1** |
| **EXPERIMENT TABLES :** | **1** |
| **CLOSED IRON RACKS :** | **1** |
| **WOODEN CLOSED RACKS :** | **1** |
| **Others:** | **STOOLS-12** |
| **LAB SPECIFICATIONS** | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **SL.NO** | **NAME OF THE EXPERIMENT** | **EQUIPMENT REQUIRED** | **EQUIPMENT** | **WORKING STATUS** |
| 1 | Determination of normal Consistency and fineness of cement. | Vicat’s apparatus AND 90MICRON Sieve | Available | Working |
|
| 2 | Determination of initial setting time and final setting time of cement | Vicat’s apparatus | Available | Working |
|
| 3 | Determination of specific gravity and soundness of cement. | specific gravity bottles and Lechatlier’s apparatus. | Available and Lechatlier apparatus not available | Working |
|
| 4 | Determination of compressive strength of cement. | compressive cube of size 70.6mmX70.6mmX70.6mm | Not available | Working |
| 5 | Determination of grading and fineness modulus of Coarse aggregate by sieve analysis. | Standard set of sieves for coarse aggregate | Available | Working |
|
| 6 | Determination of specific gravity of coarse aggregate | Wire basket and Spring Balance | available | Working |
|
| 7 | Determination of grading and fineness modulus of fine aggregate (sand) by sieve analysis. | Standard set of sieves for fine aggregate | Available | Working |
| 8 | Determination of bulking of sand. | 1000 ml jar | Available | Working |
|
| 9 | Determination of workability of concrete by compaction factor method. | Compaction factor test apparatus | Available | maintenance |
|
| 10 | Determination of workability of concrete by slump test | Slump test apparatus | Available | Working |
| 11 | Determination of workability of concrete by Vee-bee test. | vee -Bee test apparatus | not available | NO |
|
| 12 | Determination of compressive strength of cement concrete and its young’s modulus. | Compression Testing Machine | Available | Not Working |
|
| 13 | Determination of split tensile strength of concrete. | Compression Testing Machine | Available | Not Working |
|
| 14 | Non-Destructive testing on concrete (for demonstration) | Rebound Hammer | Available | Not Working |
|